/*
 * @brief Blinky Example using Dual Core communication
 *
 * @note
 * Copyright(C) NXP Semiconductors, 2013
 * All rights reserved.
 *
 * @par
 * Software that is described herein is for illustrative purposes only
 * which provides customers with programming information regarding the
 * LPC products.  This software is supplied "AS IS" without any warranties of
 * any kind, and NXP Semiconductors and its licensor disclaim any and
 * all warranties, express or implied, including all implied warranties of
 * merchantability, fitness for a particular purpose and non-infringement of
 * intellectual property rights.  NXP Semiconductors assumes no responsibility
 * or liability for the use of the software, conveys no license or rights under any
 * patent, copyright, mask work right, or any other intellectual property rights in
 * or to any products. NXP Semiconductors reserves the right to make changes
 * in the software without notification. NXP Semiconductors also makes no
 * representation or warranty that such application will be suitable for the
 * specified use without further testing or modification.
 *
 * @par
 * Permission to use, copy, modify, and distribute this software and its
 * documentation is hereby granted, under NXP Semiconductors' and its
 * licensor's relevant copyrights in the software, without fee, provided that it
 * is used in conjunction with NXP Semiconductors microcontrollers.  This
 * copyright, permission, and disclaimer notice must appear in all copies of
 * this code.
 */

/** @defgroup EXAMPLE_DUALCORE_BLINKY LPC43xx Blinky Standalone Example using Dual Core communication
 * @ingroup EXAMPLES_DUALCORE_43XX
 * <b>Example description</b><br>
 * This example blinks LED1 and LED2 at various rates, one of the LED
 * is turned on/off by M4 based on message received from M0. Meanwhile
 * M4 also sends blink message to M0 so that M0 core blinks the other LED.
 * LED1 will blink at the rate of 500ms/blink, LED2 will blink at the rate of
 * 1s/blink.<br>
 *
 * This example is included by default in all other dual-core examples,
 * hence all the dual-core examples will blink LED1 and LED2.<br>
 *
 * **IMPORTANT NOTE:**<br>
 * 
 * M0 image boot failure will also cause (by default) LED2 to blink. This
 * should not be confused with the Blinky task blinking the LED. The error
 * blink will be at 20ms or 2s rate, the former rate indicates that the M0
 * image loader code running on core-M4 could not locate a valid M0 image,
 * whereas the latter rate indicates that a valid M0 image is found but its
 * functionality is mutually exclusive with the functionalities of the image
 * running in core-M4. In case of M0 boot error the blink will stop after 1
 * minute.<br>
 *
 * <b>Special connection requirements</b><br>
 *   - Hitex LPC4350EVA-A4-2<br>
 *      + LED1 is D10 (located below micro USB connector X9, **needs jumper JP3 closed**)<br>
 *      + LED2 is RED of RGB LED<br>
 *   - KEIL MCB4357<br>
 *      + LED1 is PD_10 (located above push button P4_0)<br>
 *      + LED2 is PD_11 (located next to LED1)<br>
 *   - NGX Explorer4330<br>
 *      + LED1 is D2 (Dull Green LED)<br>
 *      + LED2 is D3 (Bright Blue LED)<br>
 *
 * <b>Build procedures:</b><br>
 * Visit the <a href="http://www.lpcware.com/content/project/lpcopen-platform-nxp-lpc-microcontrollers/lpcopen-v200-quickstart-guides">LPCOpen quickstart guides</a>
 * to get started building LPCOpen projects.
 *
 * <b>Supported boards and board setup:</b><br>
 * @ref LPCOPEN_18XX_BOARD_HITEX1850<br>
 * @ref LPCOPEN_43XX_BOARD_HITEX4350<br>
 * @ref LPCOPEN_18XX_BOARD_KEIL1857<br>
 * @ref LPCOPEN_43XX_BOARD_KEIL4357<br>
 * @ref LPCOPEN_18XX_BOARD_NGX1830<br>
 * @ref LPCOPEN_43XX_BOARD_NGX4330<br>
 *
 * <b>Submitting LPCOpen issues:</b><br>
 * @ref LPCOPEN_COMMUNITY
 * @{
 */

/**
 * @}
 */