I2S example
This example show how to use the I2S in 3 modes : Polling, Interrupt and DMA

Example description
The I2S example shows how to configure I2S and UDA1380 to receive audio signal and
play back with three modes: polling, interrupt, and DMA.

To use the example, connect a serial cable to the board's RS232/UART port and
start a terminal program to monitor the port.  The terminal program on the host
PC should be setup for 115K8N1.
For boards that has no default UART (ex: NGX Xplorer), by default example will
start in DMA mode hence no need to slect anything from terminal.
Connect the computer line out to board line-in (using 3.5mm male-to-male cable),
plug the headphone/speaker into board line-out. Change modes by selecting the
option from the terminal. Play audio on computer and listen from target board!

Special connection requirements
There are no special connection requirements for this example.

Build procedures:
Visit the <a href="http://www.lpcware.com/content/project/lpcopen-platform-nxp-lpc-microcontrollers/lpcopen-v200-quickstart-guides">LPCOpen quickstart guides</a>
to get started building LPCOpen projects.