Blinky example

Example description
Welcome to the uC/OS-III basic blinky example. This example starts up
uC/OS-III and creates 3 tasks. Tasks 1 and 2 blink different LEDs at
different rates. Task 3 outputs a tick count to the debug channel (UART)
every second.

To use the example, connect a serial cable to the board's RS232/UART port
and start a terminal program (115.2K8N1) to monitor the port. The LEDs will
also toggle based on the task execution.

Special connection requirements
There are no special connection requirements for this example.

Build procedures:
Visit the <a href="http://www.lpcware.com/content/project/lpcopen-platform-nxp-lpc-microcontrollers/lpcopen-v200-quickstart-guides">LPCOpen quickstart guides</a>
to get started building LPCOpen projects.