This file contains USB HID Mouse example using USB ROM Drivers.

Example description
The example shows how to us USBD ROM stack to creates a HID mouse.

Special connection requirements
The tiny joystick that is surface mounted on the eval board moves the mouse.
Pressing the joystick in causes a left mouse click to happening over USB.
For most OSs, no drivers are needed. If no joystick is available on the board
push button can be used to simulate a right click.

Build procedures:
Visit the <a href="http://www.lpcware.com/content/project/lpcopen-platform-nxp-lpc-microcontrollers/lpcopen-v200-quickstart-guides">LPCOpen quickstart guides</a>
to get started building LPCOpen projects.