State Configurable Timer Blinky example

Example description
This example implements the Blinky example using State Configurable Timer module.
The FSM is built by using FZM tool. The FZM tool can be downloded from : 
<a href="http://www.lpcware.com/content/nxpfile/sct-tools">SCT Tools</a>

Special connection requirements
  - Hitex LPC1850EVA-A4-2 and LPC4350EVA-A4-2 boards
    Make sure that the jumper JP34 is in 2-3 position for SCTIN_1 
  - Keil MCB1857 and MCB4357 boards

Build procedures:
Visit the <a href="http://www.lpcware.com/content/project/lpcopen-platform-nxp-lpc-microcontrollers/lpcopen-v200-quickstart-guides">LPCOpen quickstart guides</a>
to get started building LPCOpen projects.