This file contains the CDC UART/Serial Port example using USB ROM Drivers.

Example description
The example shows how to us USBD ROM stack to creates a CDC UART/Serial port bridge.
 
Special connection requirements
Connect the USB cable between micro connector on board and to a host.
When connected to Windows host use the .inf included in the project
directory to install the driver. For OSx (Mac) host no drivers is needed. 

Build procedures:
Visit the <a href="http://www.lpcware.com/content/project/lpcopen-platform-nxp-lpc-microcontrollers/lpcopen-v200-quickstart-guides">LPCOpen quickstart guides</a>
to get started building LPCOpen projects.