# Static Call Graph for image .\keil_output\periph_uart.axf

#<CALLGRAPH># ARM Linker, 5.03 [Build 76]: Last Updated: Tue Jul 07 16:27:39 2015

### Maximum Stack Usage = 164 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

__rt_entry_main ⇒ main ⇒ App_DMA_Test ⇒ Chip_GPDMA_Transfer ⇒ setupChannel

### Functions with no stack information

- __user_initial_stackheap

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- SVC_Handler ⇒ SVC_Handler
- DebugMon_Handler ⇒ DebugMon_Handler
- PendSV_Handler ⇒ PendSV_Handler
- SysTick_Handler ⇒ SysTick_Handler
- UnHandled_Vector ⇒ UnHandled_Vector
- ADC0_IRQHandler ⇒ ADC0_IRQHandler
- Chip_Clock_GetMainPLLHz ⇒ Chip_Clock_GetClockInputHz
- Chip_Clock_GetDivRate ⇒ Chip_Clock_GetClockInputHz
- _sys_exit ⇒ _sys_exit

  ### Function Pointers

  - ADC0_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - ADC1_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - ADCHS_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - ATIMER_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - BusFault_Handler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - CAN0_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - CAN1_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - DAC_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - DMA_IRQHandler from uart.o(i.DMA_IRQHandler) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - DebugMon_Handler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - ETH_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - EVRT_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - FLASH_EEPROM_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - GINT0_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - GINT1_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - GPIO0_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - GPIO1_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - GPIO2_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - GPIO3_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - GPIO4_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - GPIO5_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - GPIO6_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - GPIO7_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - HardFault_Handler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - I2C0_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - I2C1_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - I2S0_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - I2S1_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - LCD_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - M0APP_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - M0SUB_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - MCPWM_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - MemManage_Handler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - NMI_Handler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - PendSV_Handler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - QEI_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - RIT_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - RTC_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - Reset_Handler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - SCT_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - SDIO_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - SGPIO_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - SPIFI_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - SPI_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - SSP0_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - SSP1_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - SVC_Handler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - SysTick_Handler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - SystemInit from sysinit.o(i.SystemInit) referenced from keil_startup_lpc18xx43xx.o(.text)
  - TIMER0_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - TIMER1_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - TIMER2_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - TIMER3_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - UART0_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - UART1_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - UART2_IRQHandler from uart.o(i.UART2_IRQHandler) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - UART3_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - USB0_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - USB1_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - UnHandled_Vector from keil_startup_lpc18xx43xx.o(.text) referenced 7 times from keil_startup_lpc18xx43xx.o(RESET)
  - UsageFault_Handler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - WDT_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - __main from __main.o(!!!main) referenced from keil_startup_lpc18xx43xx.o(.text)

  ### Global Symbols

  __main (Thumb, 8 bytes, Stack size 0 bytes, __main.o(!!!main))
  [Calls]

  - >> __scatterload
  - >> __rt_entry

  __scatterload (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter))
  [Called By]

  - >> __main

  __scatterload_rt2 (Thumb, 44 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)
  [Calls]

  - >> __rt_entry

  __scatterload_rt2_thumb_only (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_null (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __decompress (Thumb, 100 bytes, Stack size unknown bytes, __dclz77c.o(!!dclz77c), UNUSED)

  __decompress2 (Thumb, 0 bytes, Stack size unknown bytes, __dclz77c.o(!!dclz77c), UNUSED)

  __scatterload_zeroinit (Thumb, 28 bytes, Stack size unknown bytes, __scatter_zi.o(!!handler_zi), UNUSED)

  __rt_lib_init (Thumb, 0 bytes, Stack size unknown bytes, libinit.o(.ARM.Collect$$libinit$$00000000))
  [Called By]

  - >> __rt_entry_li

  __rt_lib_init_fp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000001))
  [Calls]

  - >> _fp_init

  __rt_lib_init_alloca_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002C))

  __rt_lib_init_argv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002A))

  __rt_lib_init_atexit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000019))

  __rt_lib_init_clock_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001F))

  __rt_lib_init_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000030))

  __rt_lib_init_exceptions_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002E))

  __rt_lib_init_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001D))

  __rt_lib_init_getenv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000021))

  __rt_lib_init_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000008))

  __rt_lib_init_lc_collate_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000F))

  __rt_lib_init_lc_ctype_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000011))

  __rt_lib_init_lc_monetary_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000013))

  __rt_lib_init_lc_numeric_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000015))

  __rt_lib_init_lc_time_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000017))

  __rt_lib_init_rand_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000C))

  __rt_lib_init_return (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000031))

  __rt_lib_init_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001B))

  __rt_lib_init_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000023))

  __rt_lib_init_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000A))

  __rt_lib_shutdown (Thumb, 0 bytes, Stack size unknown bytes, libshutdown.o(.ARM.Collect$$libshutdown$$00000000))
  [Called By]

  - >> __rt_exit_ls

  __rt_lib_shutdown_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000006))

  __rt_lib_shutdown_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000E))

  __rt_lib_shutdown_return (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000F))

  __rt_lib_shutdown_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000009))

  __rt_lib_shutdown_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000003))

  __rt_lib_shutdown_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000B))

  __rt_entry (Thumb, 0 bytes, Stack size unknown bytes, rtentry.o(.ARM.Collect$$rtentry$$00000000))
  [Called By]

  - >> __scatterload_rt2
  - >> __main

  __rt_entry_presh_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$00000002))

  __rt_entry_sh (Thumb, 0 bytes, Stack size unknown bytes, rtentry4.o(.ARM.Collect$$rtentry$$00000004))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_sh ⇒ __user_setup_stackheap
  [Calls]
  - >> __user_setup_stackheap

  __rt_entry_li (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000A))
  [Calls]

  - >> __rt_lib_init

  __rt_entry_postsh_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$00000009))

  __rt_entry_main (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000D))
  [Stack]

  - Max Depth = 164 + Unknown Stack Size
  - Call Chain = __rt_entry_main ⇒ main ⇒ App_DMA_Test ⇒ Chip_GPDMA_Transfer ⇒ setupChannel
  [Calls]
  - >> main
  - >> exit

  __rt_entry_postli_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000C))

  __rt_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit.o(.ARM.Collect$$rtexit$$00000000))
  [Called By]

  - >> exit

  __rt_exit_ls (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000003))
  [Calls]

  - >> __rt_lib_shutdown

  __rt_exit_prels_1 (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000002))

  __rt_exit_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000004))
  [Calls]

  - >> _sys_exit

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - keil_startup_lpc18xx43xx.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - keil_startup_lpc18xx43xx.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - keil_startup_lpc18xx43xx.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - keil_startup_lpc18xx43xx.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - keil_startup_lpc18xx43xx.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - keil_startup_lpc18xx43xx.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Calls]

  - >> DebugMon_Handler
  [Called By]
  - >> DebugMon_Handler
  [Address Reference Count : 1]
  - keil_startup_lpc18xx43xx.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - keil_startup_lpc18xx43xx.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Calls]

  - >> SysTick_Handler
  [Called By]
  - >> SysTick_Handler
  [Address Reference Count : 1]
  - keil_startup_lpc18xx43xx.o(RESET)

  UnHandled_Vector (Thumb, 2 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Calls]

  - >> UnHandled_Vector
  [Called By]
  - >> UnHandled_Vector
  [Address Reference Count : 1]
  - keil_startup_lpc18xx43xx.o(RESET)

  ADC0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Calls]

  - >> ADC0_IRQHandler
  [Called By]
  - >> ADC0_IRQHandler
  [Address Reference Count : 1]
  - keil_startup_lpc18xx43xx.o(RESET)

  ADC1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  ADCHS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  ATIMER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  CAN0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  CAN1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  DAC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  ETH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  EVRT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  FLASH_EEPROM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  GINT0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  GINT1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  GPIO0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  GPIO1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  GPIO2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  GPIO3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  GPIO4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  GPIO5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  GPIO6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  GPIO7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  I2C0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  I2C1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  I2S0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  I2S1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  LCD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  M0APP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  M0SUB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  MCPWM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  QEI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  RIT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  SCT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  SGPIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  SPIFI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  SPI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  SSP0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  SSP1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  TIMER0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  TIMER1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  TIMER2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  TIMER3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  UART0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  UART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  UART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  USB0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  USB1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  WDT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  __user_initial_stackheap (Thumb, 0 bytes, Stack size unknown bytes, keil_startup_lpc18xx43xx.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __aeabi_memcpy (Thumb, 0 bytes, Stack size 0 bytes, rt_memcpy_v6.o(.text))
  [Called By]

  - >> RingBuffer_PopMult
  - >> RingBuffer_Pop
  - >> RingBuffer_InsertMult
  - >> RingBuffer_Insert

  __rt_memcpy (Thumb, 138 bytes, Stack size 0 bytes, rt_memcpy_v6.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memcpy4

  _memcpy_lastbytes (Thumb, 0 bytes, Stack size unknown bytes, rt_memcpy_v6.o(.text), UNUSED)

  __use_two_region_memory (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_escrow$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_expand$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __aeabi_memcpy4 (Thumb, 0 bytes, Stack size 8 bytes, rt_memcpy_w.o(.text), UNUSED)
  [Called By]

  - >> __rt_memcpy

  __aeabi_memcpy8 (Thumb, 0 bytes, Stack size 8 bytes, rt_memcpy_w.o(.text), UNUSED)

  __rt_memcpy_w (Thumb, 100 bytes, Stack size 8 bytes, rt_memcpy_w.o(.text), UNUSED)

  _memcpy_lastbytes_aligned (Thumb, 0 bytes, Stack size unknown bytes, rt_memcpy_w.o(.text), UNUSED)

  __user_setup_stackheap (Thumb, 74 bytes, Stack size 8 bytes, sys_stackheap_outer.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __user_setup_stackheap
  [Calls]
  - >> __user_initial_stackheap
  - >> __user_perproc_libspace
  [Called By]
  - >> __rt_entry_sh

  exit (Thumb, 12 bytes, Stack size 0 bytes, exit.o(.text))
  [Calls]

  - >> __rt_exit
  [Called By]
  - >> __rt_entry_main

  __user_libspace (Thumb, 8 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_perproc_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __user_perthread_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  Board_Debug_Init (Thumb, 36 bytes, Stack size 8 bytes, board.o(i.Board_Debug_Init))
  [Stack]

  - Max Depth = 88
  - Call Chain = Board_Debug_Init ⇒ Chip_UART_SetBaud ⇒ Chip_Clock_GetRate ⇒ Chip_Clock_GetBaseClocktHz ⇒ Chip_Clock_GetClockInputHz ⇒ Chip_Clock_GetMainPLLHz ⇒ Chip_Clock_GetClockInputHz (Cycle)
  [Calls]
  - >> Chip_UART_SetBaud
  - >> Chip_UART_Init
  - >> Board_UART_Init
  [Called By]
  - >> Board_Init

  Board_Init (Thumb, 128 bytes, Stack size 16 bytes, board.o(i.Board_Init))
  [Stack]

  - Max Depth = 104
  - Call Chain = Board_Init ⇒ Board_Debug_Init ⇒ Chip_UART_SetBaud ⇒ Chip_Clock_GetRate ⇒ Chip_Clock_GetBaseClocktHz ⇒ Chip_Clock_GetClockInputHz ⇒ Chip_Clock_GetMainPLLHz ⇒ Chip_Clock_GetClockInputHz (Cycle)
  [Calls]
  - >> SystemCoreClockUpdate
  - >> Chip_GPIO_Init
  - >> Board_Debug_Init
  - >> Chip_SCU_PinMuxSet
  - >> Chip_GPIO_SetPinDIROutput
  [Called By]
  - >> main

  Board_SetupClocking (Thumb, 82 bytes, Stack size 16 bytes, board_sysinit.o(i.Board_SetupClocking))
  [Stack]

  - Max Depth = 120
  - Call Chain = Board_SetupClocking ⇒ Chip_SetupCoreClock ⇒ Chip_Clock_SetupMainPLLHz ⇒ Chip_Clock_SetupMainPLLMult ⇒ Chip_Clock_GetClockInputHz ⇒ Chip_Clock_GetMainPLLHz ⇒ Chip_Clock_GetClockInputHz (Cycle)
  [Calls]
  - >> Chip_Clock_SetDivider
  - >> Chip_Clock_SetBaseClock
  - >> Chip_SetupCoreClock
  [Called By]
  - >> Board_SystemInit

  Board_SetupMuxing (Thumb, 24 bytes, Stack size 8 bytes, board_sysinit.o(i.Board_SetupMuxing))
  [Stack]

  - Max Depth = 24
  - Call Chain = Board_SetupMuxing ⇒ Chip_SCU_SetPinMuxing
  [Calls]
  - >> Chip_SCU_SetPinMuxing
  [Called By]
  - >> Board_SystemInit

  Board_SystemInit (Thumb, 14 bytes, Stack size 8 bytes, board_sysinit.o(i.Board_SystemInit))
  [Stack]

  - Max Depth = 128
  - Call Chain = Board_SystemInit ⇒ Board_SetupClocking ⇒ Chip_SetupCoreClock ⇒ Chip_Clock_SetupMainPLLHz ⇒ Chip_Clock_SetupMainPLLMult ⇒ Chip_Clock_GetClockInputHz ⇒ Chip_Clock_GetMainPLLHz ⇒ Chip_Clock_GetClockInputHz (Cycle)
  [Calls]
  - >> Board_SetupMuxing
  - >> Board_SetupClocking
  [Called By]
  - >> SystemInit

  Board_UART_Init (Thumb, 82 bytes, Stack size 8 bytes, board.o(i.Board_UART_Init))
  [Stack]

  - Max Depth = 8
  - Call Chain = Board_UART_Init
  [Calls]
  - >> Chip_SCU_PinMuxSet
  [Called By]
  - >> main
  - >> Board_Debug_Init

  Chip_Clock_Disable (Thumb, 42 bytes, Stack size 0 bytes, clock_18xx_43xx.o(i.Chip_Clock_Disable))
  [Called By]

  - >> Chip_UART_DeInit

  Chip_Clock_DisableMainPLL (Thumb, 12 bytes, Stack size 0 bytes, clock_18xx_43xx.o(i.Chip_Clock_DisableMainPLL))
  [Called By]

  - >> Chip_Clock_SetupMainPLLMult

  Chip_Clock_EnableCrystal (Thumb, 56 bytes, Stack size 8 bytes, clock_18xx_43xx.o(i.Chip_Clock_EnableCrystal))
  [Stack]

  - Max Depth = 8
  - Call Chain = Chip_Clock_EnableCrystal
  [Called By]
  - >> Chip_SetupCoreClock

  Chip_Clock_EnableOpts (Thumb, 48 bytes, Stack size 8 bytes, clock_18xx_43xx.o(i.Chip_Clock_EnableOpts))
  [Stack]

  - Max Depth = 8
  - Call Chain = Chip_Clock_EnableOpts
  [Called By]
  - >> Chip_UART_Init
  - >> Chip_GPDMA_Init

  Chip_Clock_GetBaseClock (Thumb, 26 bytes, Stack size 0 bytes, clock_18xx_43xx.o(i.Chip_Clock_GetBaseClock))
  [Called By]

  - >> Chip_Clock_GetBaseClocktHz

  Chip_Clock_GetBaseClocktHz (Thumb, 14 bytes, Stack size 8 bytes, clock_18xx_43xx.o(i.Chip_Clock_GetBaseClocktHz))
  [Stack]

  - Max Depth = 40
  - Call Chain = Chip_Clock_GetBaseClocktHz ⇒ Chip_Clock_GetClockInputHz ⇒ Chip_Clock_GetMainPLLHz ⇒ Chip_Clock_GetClockInputHz (Cycle)
  [Calls]
  - >> Chip_Clock_GetClockInputHz
  - >> Chip_Clock_GetBaseClock
  [Called By]
  - >> Chip_Clock_GetRate

  Chip_Clock_GetClockInputHz (Thumb, 132 bytes, Stack size 8 bytes, clock_18xx_43xx.o(i.Chip_Clock_GetClockInputHz))
  [Stack]

  - Max Depth = 32
  - Call Chain = Chip_Clock_GetClockInputHz ⇒ Chip_Clock_GetMainPLLHz ⇒ Chip_Clock_GetClockInputHz (Cycle)
  [Calls]
  - >> Chip_Clock_GetMainPLLHz
  - >> Chip_Clock_GetDivRate
  [Called By]
  - >> Chip_Clock_SetupMainPLLMult
  - >> Chip_Clock_SetupMainPLLHz
  - >> Chip_Clock_GetMainPLLHz
  - >> Chip_Clock_GetBaseClocktHz
  - >> Chip_Clock_GetDivRate

  Chip_Clock_GetDividerDivisor (Thumb, 18 bytes, Stack size 0 bytes, clock_18xx_43xx.o(i.Chip_Clock_GetDividerDivisor))
  [Called By]

  - >> Chip_Clock_GetDivRate

  Chip_Clock_GetDividerSource (Thumb, 22 bytes, Stack size 0 bytes, clock_18xx_43xx.o(i.Chip_Clock_GetDividerSource))
  [Called By]

  - >> Chip_Clock_GetDivRate

  Chip_Clock_GetMainPLLHz (Thumb, 84 bytes, Stack size 24 bytes, clock_18xx_43xx.o(i.Chip_Clock_GetMainPLLHz))
  [Stack]

  - Max Depth = 24 + In Cycle
  - Call Chain = Chip_Clock_GetMainPLLHz ⇒ Chip_Clock_GetClockInputHz (Cycle)
  [Calls]
  - >> Chip_Clock_GetClockInputHz
  [Called By]
  - >> Chip_Clock_GetClockInputHz

  Chip_Clock_GetRate (Thumb, 112 bytes, Stack size 24 bytes, clock_18xx_43xx.o(i.Chip_Clock_GetRate))
  [Stack]

  - Max Depth = 64
  - Call Chain = Chip_Clock_GetRate ⇒ Chip_Clock_GetBaseClocktHz ⇒ Chip_Clock_GetClockInputHz ⇒ Chip_Clock_GetMainPLLHz ⇒ Chip_Clock_GetClockInputHz (Cycle)
  [Calls]
  - >> Chip_Clock_GetBaseClocktHz
  [Called By]
  - >> SystemCoreClockUpdate
  - >> Chip_UART_SetBaud

  Chip_Clock_SetBaseClock (Thumb, 48 bytes, Stack size 12 bytes, clock_18xx_43xx.o(i.Chip_Clock_SetBaseClock))
  [Stack]

  - Max Depth = 12
  - Call Chain = Chip_Clock_SetBaseClock
  [Called By]
  - >> Chip_SetupCoreClock
  - >> Board_SetupClocking

  Chip_Clock_SetDivider (Thumb, 50 bytes, Stack size 12 bytes, clock_18xx_43xx.o(i.Chip_Clock_SetDivider))
  [Stack]

  - Max Depth = 12
  - Call Chain = Chip_Clock_SetDivider
  [Called By]
  - >> Board_SetupClocking

  Chip_Clock_SetupMainPLLHz (Thumb, 130 bytes, Stack size 32 bytes, clock_18xx_43xx.o(i.Chip_Clock_SetupMainPLLHz))
  [Stack]

  - Max Depth = 88
  - Call Chain = Chip_Clock_SetupMainPLLHz ⇒ Chip_Clock_SetupMainPLLMult ⇒ Chip_Clock_GetClockInputHz ⇒ Chip_Clock_GetMainPLLHz ⇒ Chip_Clock_GetClockInputHz (Cycle)
  [Calls]
  - >> Chip_Clock_GetClockInputHz
  - >> Chip_Clock_SetupMainPLLMult
  - >> Chip_Clock_TestMainPLLMultiplier
  [Called By]
  - >> Chip_SetupCoreClock

  Chip_Clock_SetupMainPLLMult (Thumb, 120 bytes, Stack size 24 bytes, clock_18xx_43xx.o(i.Chip_Clock_SetupMainPLLMult))
  [Stack]

  - Max Depth = 56
  - Call Chain = Chip_Clock_SetupMainPLLMult ⇒ Chip_Clock_GetClockInputHz ⇒ Chip_Clock_GetMainPLLHz ⇒ Chip_Clock_GetClockInputHz (Cycle)
  [Calls]
  - >> Chip_Clock_GetClockInputHz
  - >> Chip_Clock_DisableMainPLL
  [Called By]
  - >> Chip_Clock_SetupMainPLLHz

  Chip_GPDMA_ChannelCmd (Thumb, 28 bytes, Stack size 0 bytes, gpdma_18xx_43xx.o(i.Chip_GPDMA_ChannelCmd))
  [Called By]

  - >> Chip_GPDMA_Transfer
  - >> Chip_GPDMA_Stop

  Chip_GPDMA_ClearIntPending (Thumb, 16 bytes, Stack size 0 bytes, gpdma_18xx_43xx.o(i.Chip_GPDMA_ClearIntPending))
  [Called By]

  - >> Chip_GPDMA_Stop
  - >> Chip_GPDMA_Interrupt

  Chip_GPDMA_GetFreeChannel (Thumb, 44 bytes, Stack size 16 bytes, gpdma_18xx_43xx.o(i.Chip_GPDMA_GetFreeChannel))
  [Stack]

  - Max Depth = 16
  - Call Chain = Chip_GPDMA_GetFreeChannel
  [Calls]
  - >> Chip_GPDMA_IntGetStatus
  [Called By]
  - >> App_DMA_Test

  Chip_GPDMA_Init (Thumb, 56 bytes, Stack size 8 bytes, gpdma_18xx_43xx.o(i.Chip_GPDMA_Init))
  [Stack]

  - Max Depth = 16
  - Call Chain = Chip_GPDMA_Init ⇒ Chip_Clock_EnableOpts
  [Calls]
  - >> Chip_Clock_EnableOpts
  [Called By]
  - >> App_DMA_Test

  Chip_GPDMA_InitChannelCfg (Thumb, 94 bytes, Stack size 20 bytes, gpdma_18xx_43xx.o(i.Chip_GPDMA_InitChannelCfg))
  [Stack]

  - Max Depth = 20
  - Call Chain = Chip_GPDMA_InitChannelCfg
  [Called By]
  - >> Chip_GPDMA_Transfer

  Chip_GPDMA_IntGetStatus (Thumb, 46 bytes, Stack size 0 bytes, gpdma_18xx_43xx.o(i.Chip_GPDMA_IntGetStatus))
  [Called By]

  - >> Chip_GPDMA_Stop
  - >> Chip_GPDMA_Interrupt
  - >> Chip_GPDMA_GetFreeChannel

  Chip_GPDMA_Interrupt (Thumb, 66 bytes, Stack size 12 bytes, gpdma_18xx_43xx.o(i.Chip_GPDMA_Interrupt))
  [Stack]

  - Max Depth = 12
  - Call Chain = Chip_GPDMA_Interrupt
  [Calls]
  - >> Chip_GPDMA_IntGetStatus
  - >> Chip_GPDMA_ClearIntPending
  [Called By]
  - >> DMA_IRQHandler

  Chip_GPDMA_Stop (Thumb, 64 bytes, Stack size 12 bytes, gpdma_18xx_43xx.o(i.Chip_GPDMA_Stop))
  [Stack]

  - Max Depth = 12
  - Call Chain = Chip_GPDMA_Stop
  [Calls]
  - >> Chip_GPDMA_IntGetStatus
  - >> Chip_GPDMA_ClearIntPending
  - >> Chip_GPDMA_ChannelCmd
  [Called By]
  - >> App_DMA_Test

  Chip_GPDMA_Transfer (Thumb, 140 bytes, Stack size 72 bytes, gpdma_18xx_43xx.o(i.Chip_GPDMA_Transfer))
  [Stack]

  - Max Depth = 92
  - Call Chain = Chip_GPDMA_Transfer ⇒ setupChannel
  [Calls]
  - >> setupChannel
  - >> makeCtrlWord
  - >> Chip_GPDMA_InitChannelCfg
  - >> Chip_GPDMA_ChannelCmd
  - >> configDMAMux
  [Called By]
  - >> App_DMA_Test

  Chip_GPIO_Init (Thumb, 2 bytes, Stack size 0 bytes, gpio_18xx_43xx.o(i.Chip_GPIO_Init))
  [Called By]

  - >> Board_Init

  Chip_SetupCoreClock (Thumb, 106 bytes, Stack size 16 bytes, sysinit_18xx_43xx.o(i.Chip_SetupCoreClock))
  [Stack]

  - Max Depth = 104
  - Call Chain = Chip_SetupCoreClock ⇒ Chip_Clock_SetupMainPLLHz ⇒ Chip_Clock_SetupMainPLLMult ⇒ Chip_Clock_GetClockInputHz ⇒ Chip_Clock_GetMainPLLHz ⇒ Chip_Clock_GetClockInputHz (Cycle)
  [Calls]
  - >> Chip_Clock_SetBaseClock
  - >> Chip_Clock_SetupMainPLLHz
  - >> Chip_Clock_EnableCrystal
  [Called By]
  - >> Board_SetupClocking

  Chip_UART_ABCmd (Thumb, 56 bytes, Stack size 8 bytes, uart_18xx_43xx.o(i.Chip_UART_ABCmd))
  [Stack]

  - Max Depth = 8
  - Call Chain = Chip_UART_ABCmd
  [Called By]
  - >> main

  Chip_UART_CheckBusy (Thumb, 14 bytes, Stack size 0 bytes, uart_18xx_43xx.o(i.Chip_UART_CheckBusy))
  [Called By]

  - >> main

  Chip_UART_DeInit (Thumb, 18 bytes, Stack size 8 bytes, uart_18xx_43xx.o(i.Chip_UART_DeInit))
  [Stack]

  - Max Depth = 8
  - Call Chain = Chip_UART_DeInit
  [Calls]
  - >> Chip_UART_GetClockIndex
  - >> Chip_Clock_Disable
  [Called By]
  - >> main

  Chip_UART_GetABEOStatus (Thumb, 6 bytes, Stack size 0 bytes, uart_18xx_43xx.o(i.Chip_UART_GetABEOStatus))
  [Called By]

  - >> main

  Chip_UART_IRQRBHandler (Thumb, 102 bytes, Stack size 16 bytes, uart_18xx_43xx.o(i.Chip_UART_IRQRBHandler))
  [Stack]

  - Max Depth = 48
  - Call Chain = Chip_UART_IRQRBHandler ⇒ Chip_UART_TXIntHandlerRB ⇒ RingBuffer_Pop
  [Calls]
  - >> RingBuffer_IsEmpty
  - >> Chip_UART_TXIntHandlerRB
  - >> Chip_UART_RXIntHandlerRB
  [Called By]
  - >> UART2_IRQHandler

  Chip_UART_Init (Thumb, 58 bytes, Stack size 8 bytes, uart_18xx_43xx.o(i.Chip_UART_Init))
  [Stack]

  - Max Depth = 16
  - Call Chain = Chip_UART_Init ⇒ Chip_Clock_EnableOpts
  [Calls]
  - >> Chip_UART_GetClockIndex
  - >> Chip_Clock_EnableOpts
  [Called By]
  - >> main
  - >> Board_Debug_Init

  Chip_UART_RXIntHandlerRB (Thumb, 30 bytes, Stack size 16 bytes, uart_18xx_43xx.o(i.Chip_UART_RXIntHandlerRB))
  [Stack]

  - Max Depth = 32
  - Call Chain = Chip_UART_RXIntHandlerRB ⇒ RingBuffer_Insert
  [Calls]
  - >> RingBuffer_Insert
  [Called By]
  - >> Chip_UART_IRQRBHandler

  Chip_UART_Read (Thumb, 28 bytes, Stack size 8 bytes, uart_18xx_43xx.o(i.Chip_UART_Read))
  [Stack]

  - Max Depth = 8
  - Call Chain = Chip_UART_Read
  [Called By]
  - >> main

  Chip_UART_ReadRB (Thumb, 16 bytes, Stack size 8 bytes, uart_18xx_43xx.o(i.Chip_UART_ReadRB))
  [Stack]

  - Max Depth = 40
  - Call Chain = Chip_UART_ReadRB ⇒ RingBuffer_PopMult
  [Calls]
  - >> RingBuffer_PopMult
  [Called By]
  - >> App_Interrupt_Test

  Chip_UART_Send (Thumb, 28 bytes, Stack size 8 bytes, uart_18xx_43xx.o(i.Chip_UART_Send))
  [Stack]

  - Max Depth = 8
  - Call Chain = Chip_UART_Send
  [Called By]
  - >> Chip_UART_SendBlocking

  Chip_UART_SendBlocking (Thumb, 36 bytes, Stack size 20 bytes, uart_18xx_43xx.o(i.Chip_UART_SendBlocking))
  [Stack]

  - Max Depth = 28
  - Call Chain = Chip_UART_SendBlocking ⇒ Chip_UART_Send
  [Calls]
  - >> Chip_UART_Send
  [Called By]
  - >> main
  - >> Print_Menu_Polling

  Chip_UART_SendRB (Thumb, 64 bytes, Stack size 24 bytes, uart_18xx_43xx.o(i.Chip_UART_SendRB))
  [Stack]

  - Max Depth = 56
  - Call Chain = Chip_UART_SendRB ⇒ RingBuffer_InsertMult
  [Calls]
  - >> RingBuffer_InsertMult
  - >> Chip_UART_TXIntHandlerRB
  [Called By]
  - >> App_Interrupt_Test

  Chip_UART_SetBaud (Thumb, 58 bytes, Stack size 16 bytes, uart_18xx_43xx.o(i.Chip_UART_SetBaud))
  [Stack]

  - Max Depth = 80
  - Call Chain = Chip_UART_SetBaud ⇒ Chip_Clock_GetRate ⇒ Chip_Clock_GetBaseClocktHz ⇒ Chip_Clock_GetClockInputHz ⇒ Chip_Clock_GetMainPLLHz ⇒ Chip_Clock_GetClockInputHz (Cycle)
  [Calls]
  - >> Chip_UART_GetClockIndex
  - >> Chip_Clock_GetRate
  [Called By]
  - >> main
  - >> Board_Debug_Init

  Chip_UART_TXIntHandlerRB (Thumb, 52 bytes, Stack size 16 bytes, uart_18xx_43xx.o(i.Chip_UART_TXIntHandlerRB))
  [Stack]

  - Max Depth = 32
  - Call Chain = Chip_UART_TXIntHandlerRB ⇒ RingBuffer_Pop
  [Calls]
  - >> RingBuffer_IsEmpty
  - >> RingBuffer_Pop
  [Called By]
  - >> Chip_UART_SendRB
  - >> Chip_UART_IRQRBHandler

  DMA_IRQHandler (Thumb, 40 bytes, Stack size 8 bytes, uart.o(i.DMA_IRQHandler))
  [Stack]

  - Max Depth = 20
  - Call Chain = DMA_IRQHandler ⇒ Chip_GPDMA_Interrupt
  [Calls]
  - >> Chip_GPDMA_Interrupt
  [Address Reference Count : 1]
  - keil_startup_lpc18xx43xx.o(RESET)

  RingBuffer_Init (Thumb, 16 bytes, Stack size 0 bytes, ring_buffer.o(i.RingBuffer_Init))
  [Called By]

  - >> App_Interrupt_Test

  RingBuffer_Insert (Thumb, 48 bytes, Stack size 16 bytes, ring_buffer.o(i.RingBuffer_Insert))
  [Stack]

  - Max Depth = 16
  - Call Chain = RingBuffer_Insert
  [Calls]
  - >> RingBuffer_IsFull
  - >> __aeabi_memcpy
  [Called By]
  - >> Chip_UART_RXIntHandlerRB

  RingBuffer_InsertMult (Thumb, 122 bytes, Stack size 32 bytes, ring_buffer.o(i.RingBuffer_InsertMult))
  [Stack]

  - Max Depth = 32
  - Call Chain = RingBuffer_InsertMult
  [Calls]
  - >> RingBuffer_IsFull
  - >> __aeabi_memcpy
  [Called By]
  - >> Chip_UART_SendRB

  RingBuffer_Pop (Thumb, 48 bytes, Stack size 16 bytes, ring_buffer.o(i.RingBuffer_Pop))
  [Stack]

  - Max Depth = 16
  - Call Chain = RingBuffer_Pop
  [Calls]
  - >> RingBuffer_IsEmpty
  - >> __aeabi_memcpy
  [Called By]
  - >> Chip_UART_TXIntHandlerRB

  RingBuffer_PopMult (Thumb, 118 bytes, Stack size 32 bytes, ring_buffer.o(i.RingBuffer_PopMult))
  [Stack]

  - Max Depth = 32
  - Call Chain = RingBuffer_PopMult
  [Calls]
  - >> RingBuffer_IsEmpty
  - >> __aeabi_memcpy
  [Called By]
  - >> Chip_UART_ReadRB

  SystemCoreClockUpdate (Thumb, 14 bytes, Stack size 8 bytes, chip_18xx_43xx.o(i.SystemCoreClockUpdate))
  [Stack]

  - Max Depth = 72
  - Call Chain = SystemCoreClockUpdate ⇒ Chip_Clock_GetRate ⇒ Chip_Clock_GetBaseClocktHz ⇒ Chip_Clock_GetClockInputHz ⇒ Chip_Clock_GetMainPLLHz ⇒ Chip_Clock_GetClockInputHz (Cycle)
  [Calls]
  - >> Chip_Clock_GetRate
  [Called By]
  - >> Board_Init
  - >> main

  SystemInit (Thumb, 20 bytes, Stack size 8 bytes, sysinit.o(i.SystemInit))
  [Stack]

  - Max Depth = 136
  - Call Chain = SystemInit ⇒ Board_SystemInit ⇒ Board_SetupClocking ⇒ Chip_SetupCoreClock ⇒ Chip_Clock_SetupMainPLLHz ⇒ Chip_Clock_SetupMainPLLMult ⇒ Chip_Clock_GetClockInputHz ⇒ Chip_Clock_GetMainPLLHz ⇒ Chip_Clock_GetClockInputHz (Cycle)
  [Calls]
  - >> fpuInit
  - >> Board_SystemInit
  [Address Reference Count : 1]
  - keil_startup_lpc18xx43xx.o(.text)

  UART2_IRQHandler (Thumb, 12 bytes, Stack size 0 bytes, uart.o(i.UART2_IRQHandler))
  [Stack]

  - Max Depth = 48
  - Call Chain = UART2_IRQHandler ⇒ Chip_UART_IRQRBHandler ⇒ Chip_UART_TXIntHandlerRB ⇒ RingBuffer_Pop
  [Calls]
  - >> Chip_UART_IRQRBHandler
  [Address Reference Count : 1]
  - keil_startup_lpc18xx43xx.o(RESET)

  _sys_exit (Thumb, 4 bytes, Stack size 0 bytes, board.o(i._sys_exit))
  [Calls]

  - >> _sys_exit
  [Called By]
  - >> _sys_exit
  - >> __rt_exit_exit

  fpuInit (Thumb, 46 bytes, Stack size 12 bytes, fpu_init.o(i.fpuInit))
  [Stack]

  - Max Depth = 12
  - Call Chain = fpuInit
  [Called By]
  - >> SystemInit

  main (Thumb, 266 bytes, Stack size 24 bytes, uart.o(i.main))
  [Stack]

  - Max Depth = 164
  - Call Chain = main ⇒ App_DMA_Test ⇒ Chip_GPDMA_Transfer ⇒ setupChannel
  [Calls]
  - >> SystemCoreClockUpdate
  - >> Chip_UART_SetBaud
  - >> Chip_UART_SendBlocking
  - >> Chip_UART_Read
  - >> Chip_UART_Init
  - >> Chip_UART_GetABEOStatus
  - >> Chip_UART_DeInit
  - >> Chip_UART_CheckBusy
  - >> Chip_UART_ABCmd
  - >> Board_UART_Init
  - >> Board_Init
  - >> Print_Menu_Polling
  - >> NVIC_SetPriority
  - >> NVIC_EnableIRQ
  - >> NVIC_DisableIRQ
  - >> App_Interrupt_Test
  - >> App_DMA_Test
  [Called By]
  - >> __rt_entry_main

  makeCtrlWord (Thumb, 140 bytes, Stack size 20 bytes, gpdma_18xx_43xx.o(i.makeCtrlWord))
  [Stack]

  - Max Depth = 20
  - Call Chain = makeCtrlWord
  [Called By]
  - >> Chip_GPDMA_Transfer

  setupChannel (Thumb, 102 bytes, Stack size 20 bytes, gpdma_18xx_43xx.o(i.setupChannel))
  [Stack]

  - Max Depth = 20
  - Call Chain = setupChannel
  [Called By]
  - >> Chip_GPDMA_Transfer

  _fp_init (Thumb, 10 bytes, Stack size 0 bytes, fpinit.o(x$fpl$fpinit))
  [Called By]

  - >> __rt_lib_init_fp_1

  __fplib_config_fpu_vfp (Thumb, 0 bytes, Stack size unknown bytes, fpinit.o(x$fpl$fpinit), UNUSED)

  __fplib_config_pureend_doubles (Thumb, 0 bytes, Stack size unknown bytes, fpinit.o(x$fpl$fpinit), UNUSED)

  ### Local Symbols

  App_DMA_Test (Thumb, 182 bytes, Stack size 48 bytes, uart.o(i.App_DMA_Test))
  [Stack]

  - Max Depth = 140
  - Call Chain = App_DMA_Test ⇒ Chip_GPDMA_Transfer ⇒ setupChannel
  [Calls]
  - >> Chip_GPDMA_Transfer
  - >> Chip_GPDMA_Stop
  - >> Chip_GPDMA_Init
  - >> Chip_GPDMA_GetFreeChannel
  - >> NVIC_SetPriority
  - >> NVIC_EnableIRQ
  - >> NVIC_DisableIRQ
  [Called By]
  - >> main

  App_Interrupt_Test (Thumb, 166 bytes, Stack size 16 bytes, uart.o(i.App_Interrupt_Test))
  [Stack]

  - Max Depth = 72
  - Call Chain = App_Interrupt_Test ⇒ Chip_UART_SendRB ⇒ RingBuffer_InsertMult
  [Calls]
  - >> RingBuffer_Init
  - >> Chip_UART_SendRB
  - >> Chip_UART_ReadRB
  - >> NVIC_SetPriority
  - >> NVIC_EnableIRQ
  - >> NVIC_DisableIRQ
  [Called By]
  - >> main

  NVIC_DisableIRQ (Thumb, 24 bytes, Stack size 0 bytes, uart.o(i.NVIC_DisableIRQ))
  [Called By]

  - >> main
  - >> App_Interrupt_Test
  - >> App_DMA_Test

  NVIC_EnableIRQ (Thumb, 24 bytes, Stack size 0 bytes, uart.o(i.NVIC_EnableIRQ))
  [Called By]

  - >> main
  - >> App_Interrupt_Test
  - >> App_DMA_Test

  NVIC_SetPriority (Thumb, 22 bytes, Stack size 0 bytes, uart.o(i.NVIC_SetPriority))
  [Called By]

  - >> main
  - >> App_Interrupt_Test
  - >> App_DMA_Test

  Print_Menu_Polling (Thumb, 42 bytes, Stack size 8 bytes, uart.o(i.Print_Menu_Polling))
  [Stack]

  - Max Depth = 36
  - Call Chain = Print_Menu_Polling ⇒ Chip_UART_SendBlocking ⇒ Chip_UART_Send
  [Calls]
  - >> Chip_UART_SendBlocking
  [Called By]
  - >> main

  configDMAMux (Thumb, 216 bytes, Stack size 12 bytes, gpdma_18xx_43xx.o(i.configDMAMux))
  [Stack]

  - Max Depth = 12
  - Call Chain = configDMAMux
  [Called By]
  - >> Chip_GPDMA_Transfer

  Chip_UART_GetClockIndex (Thumb, 34 bytes, Stack size 0 bytes, uart_18xx_43xx.o(i.Chip_UART_GetClockIndex))
  [Called By]

  - >> Chip_UART_SetBaud
  - >> Chip_UART_Init
  - >> Chip_UART_DeInit

  RingBuffer_IsEmpty (Thumb, 16 bytes, Stack size 0 bytes, uart_18xx_43xx.o(i.RingBuffer_IsEmpty))
  [Called By]

  - >> Chip_UART_IRQRBHandler
  - >> Chip_UART_TXIntHandlerRB

  RingBuffer_IsEmpty (Thumb, 16 bytes, Stack size 0 bytes, ring_buffer.o(i.RingBuffer_IsEmpty))
  [Called By]

  - >> RingBuffer_PopMult
  - >> RingBuffer_Pop

  RingBuffer_IsFull (Thumb, 20 bytes, Stack size 0 bytes, ring_buffer.o(i.RingBuffer_IsFull))
  [Called By]

  - >> RingBuffer_InsertMult
  - >> RingBuffer_Insert

  Chip_GPIO_SetPinDIROutput (Thumb, 20 bytes, Stack size 0 bytes, board.o(i.Chip_GPIO_SetPinDIROutput))
  [Called By]

  - >> Board_Init

  Chip_SCU_PinMuxSet (Thumb, 12 bytes, Stack size 0 bytes, board.o(i.Chip_SCU_PinMuxSet))
  [Called By]

  - >> Board_UART_Init
  - >> Board_Init

  Chip_SCU_SetPinMuxing (Thumb, 36 bytes, Stack size 16 bytes, board_sysinit.o(i.Chip_SCU_SetPinMuxing))
  [Stack]

  - Max Depth = 16
  - Call Chain = Chip_SCU_SetPinMuxing
  [Called By]
  - >> Board_SetupMuxing

  Chip_Clock_GetDivRate (Thumb, 34 bytes, Stack size 8 bytes, clock_18xx_43xx.o(i.Chip_Clock_GetDivRate))
  [Stack]

  - Max Depth = 8 + In Cycle
  - Call Chain = Chip_Clock_GetDivRate ⇒ Chip_Clock_GetClockInputHz (Cycle)
  [Calls]
  - >> Chip_Clock_GetClockInputHz
  - >> Chip_Clock_GetDividerSource
  - >> Chip_Clock_GetDividerDivisor
  [Called By]
  - >> Chip_Clock_GetClockInputHz

  Chip_Clock_TestMainPLLMultiplier (Thumb, 20 bytes, Stack size 0 bytes, clock_18xx_43xx.o(i.Chip_Clock_TestMainPLLMultiplier))
  [Called By]

  - >> Chip_Clock_SetupMainPLLHz

  ### Undefined Global Symbols