
Purpose:
	This is a simple example for Watchdog timer application in interrupt mode
	Using UART0 with this configuration – 115200bps – 8 data bit – No parity – 1 stop bit – No flow control 


Hardware configuration:
	This example tested on Keil MCB1700 vers.1
	These jumpers must be configured as following:
		- VDDIO, VDDREGS, VBUS, LED must be closed.

Running mode:
	This example can run on RAM mode with a debugger or run on FLASH after burning.
	
Note:
	None