This is a HTTP Server example. It shows how to use the
Web Server CGI interface. 

Use this example to connect MCB1700 Board to a LAN with DHCP
server (most LANs have this). This example will configure the 
LAN network parameters automatically using a DHCP protocol.

You may connect MCB1700 Board to PC directly over a crosslink
network cable. In this case configure a PC to use a static 
IP address 192.168.0.1

If after a timeout of 5 seconds DHCP did not obtain an IP address,
this example will use a static IP address 192.168.0.100

The WEB pages are included into the project under HTTP Files 
group. You can simply add or remove a page or image. Web files
which are compiled into the project are added to the 'Web.inp'
Web Converter input file.

To test this example, open your web browser and enter the 
address http://mcb1700/ or http://<boards IP address>

Default user    : admin
Default password: <none>

You can change the password at runtime on page 'system'

The HTTP_demo example is available for several targets:

MCB1700:       Standalone (no RTX Kernel) application.
               Program code is loaded into on-chip flash.

MCB1700 Debug: Standalone (no RTX Kernel) with debug output.
               Debug level configured in Net_Debug.c configuration file.
               Connect a serial cable to RS232 COM1 port using
               HyperTerminal at 115200 baud, 8-bits, no parity,
               1 stop bit, flowcontrol none.

MCB1700 RTX:   The same example configured for RTX Kernel.