Purpose:
	This is a simple example to test CAN transfer data between two board

	Using UART0 with this configuration:
		– 115200bps 
		– 8 data bits
		– No parity 
		– 1 stop bit 
		– No flow control 
	
Hardware configuration:
        This example runs on IAR-LPC1768-SK or Keil MCB2300 platform v4.0 with LPC1768
        IAR-LPC1768-SK configuration
          - CAN_H on the firts board conected to CAN_H on the second doard
          - CAN_L on the firts board conected to CAN_L on the second doard
          - GND on the firts board conected to GND on the second doard
        KEIL board configuration
          - CAN1-Pin2 on the first board connects to CAN1-Pin2 on the second board.
          - CAN1-Pin7 on the first board connects to CAN1-Pin7 on the second board.	
	
Running mode:
        Run the transmit programe on first board on FLASH mode.
        Run the receive programe on second board on RAM mode with debugger.
	
Note:
        - If you want to chose Transmit or Receive programe, check via macro "CAN_TRANSMIT"