This is a modified version of the NXP CMSIS Driver Library. The following changes were implemented:

1. All examples use a common library. Common options are included in Drivers/include/lpc17xx_libcfg.h.

2. The DEBUG function check_failed() is now on micromint/src/debug.h instead of being part of every example.

3. The example names were changes as follows:

    Current     NXP CMSIS

    blinky      GPIO\LedBlinky
    uart_echo   UART\interrupt

4. There is an IAR workspace that includes examples. TODO: CodeBlocks and Eclipse workspaces.
